## Winding Layout – Electric Motor RPII Pumps

A diagram of a diagram of a star connection

Description automatically generated

Winding parameters

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| Slots | 12 |
| Phases | 3 |
| Turns per Coil | 3 |
| Wires at Hand | 14 |
| Wire diameter (IEC-60317-13) [mm] | 0.75 |
| Coil pitch | 2 |
| Layers | 2 |
| Parallel paths | 1 |